|  |  |  |
| --- | --- | --- |
| Product Catalogue | D-Sub/DVI/HDMI connector |  |
| Connector Type | D-Sub |  |
| Male-Female | Male |  |
| Total Number of Pins | 9 |  |
| Row Number | 2 |  |
| Installation method | Bend insertion |  |
| Rated current | 5A |  |
| Working temperature range | -55℃~+105℃ |  |
| Welding temperature (maximum value) | 260℃ |  |

<https://item.szlcsc.com/3216208.html>